**Appendix A**

(Description of Work Scope Items)

**Wooden Pier Supports & Dead-head Removal:**

Area 1: Wooden Pier Support Removal (see pictures for project scope)

Area 2: Dead-head Removal (see pictures for project scope)

Contractors must visit site to determine quantities for removal (sole responsibility of contractor). A pre-bid site visit with the Conservation District can be arranged by calling

(906) 553-7700 and leaving your contact information (please schedule ahead).

Wooden supports and dead-heads must be cut off and removed to the riverbed.

**Cement Abutment Removal:**

Area 3: Cement Abutments Removal (see pictures for project scope)

Contractors must visit site to determine quantities for removal (sole responsibility of contractor). A pre-bid site visit with the Conservation District can be arranged by calling

(906) 553-7700 and leaving your contact information (please schedule ahead).

All cement abutments are 4ft. by 10 ft.

1. 8 ft. high
2. 12 ft. high
3. 15 ft. high
4. 25 ft. high

Cement abutments and supports must be removed to the riverbed.

**Other Available Information**

**No coffer-dams or roadways are permitted for removal – Barge use only.**

**Clearance of 15 ft. plus between Railroad bridge and river.**

**Railroad crossing easement for loading equipment onto barge can be applied for to EL&S RR for permit fees of approx. $4,000.00 (contractor responsibility).**

**MDEQ & Corps Permits must be followed.**

**For this contract schedule of values can only divide pay items into work scope items for those Bid items:**

1. **Wooden Pier Supports & Dead-head Removal**
2. **Cement Abutment Removal**

**Request for payment on work scope items can only be done after each scope of work Bid item under “Bid Schedule” is complete.**